,Catalog Number##other##,Lamp Type##other##,Wattage##other##,Conduit Size##Length##inches,Shipping Weight##other##,Ballast Housing##other##,Outlet Box##other##,Globe##other##,Guard##other##,Photometric Web File##other##,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN
03-S-04-GG-C,SAFJ05-H-04-GG-C,High Pressure Sodium,35,0.75,12.5,SAFJ03S04,JMP,JGL15,JGU15,generic,3000
03-S-04-GG-C1,SAFJ03-S-04-GG-C1,High Pressure Sodium,35,1.00,12.5,SAFJ03S04,JMP1,JGL15,JGU15,generic,3000
05-S-04-GG-C,SAFJ05-S-04-GG-C,High Pressure Sodium,50,0.75,13.5,SAFJ05S04,JMP,JGL15,JGU15,SAFJ05S.IES,3000
05-S-04-GG-C1,SAFJ05-S-04-GG-C1,High Pressure Sodium,50,1.00,13.5,SAFJ05S04,JMP1,JGL15,JGU15,SAFJ05S.IES,3000
07-S-04-GG-C,SAFJ07-S-04-GG-C,High Pressure Sodium,70,0.75,14.5,SAFJ07S04,JMP,JGL15,JGU15,SAFJ07S.IES,3000
07-S-04-GG-C1,SAFJ07-S-04-GG-C1,High Pressure Sodium,70,1.00,14.5,SAFJ07S04,,JGL15,JGU15,SAFJ07S.IES,3000
10-S-04-GG-C,SAFJ10-S-04-GG-C,High Pressure Sodium,100,0.75,16.5,SAFJ010S04,JMP1,JGL15,JGU15,SAFJ10S.ies,3000
10-S-04-GG-C1,SAFJ10-S-04-GG-C1,High Pressure Sodium,100,1.00,16.5,SAFJ010S04,JMP,JGL15,JGU15,SAFJ10S.ies,3000
05-H-04-GG-C,SAFJ05-H-04-GG-C,Metal Halide,50,0.75,14,SAFJ05H04,JMC,JGL15,JGU15,SAFJ05S.IES,4000
05-H-04-GG-C1,SAFJ05-H-04-GG-C1,Metal Halide,50,1.00,14,SAFJ05H04,JMC1,JGL15,JGU15,SAFJ05S.IES,4000
07-H-04-GG-C,SAFJ07-H-04-GG-C,Metal Halide,70,0.75,14,SAFJ07H04,JMC,JGL15,JGU15,SAFJ07S.IES,4000
07-H-04-GG-C1,SAFJ07-H-04-GG-C1,Metal Halide,70,1.00,14,SAFJ07H04,JMC1,JGL15,JGU15,SAFJ07S.IES,4000
10-H-04-GG-C,SAFJ10-H-04-GG-C,Metal Halide,100,0.75,15,SAFJ10H04,JMC,JGL15,JGU15,SAFJ10S.ies,4000
10-H-04-GG-C1,SAFJ10-H-04-GG-C1,Metal Halide,100,1.00,15,SAFJ10H04,JMC1,JGL15,JGU15,SAFJ10S.ies,4000
