,Catalog Number##other##,Lamp Type##other##,Watt##other##,Conduit Size##Length##inches,Shipping Weight##other##,Ballast Housing##other##,Outlet Box##other##,Globe##other##,Guard##other##,Photometric Web File##other##,Rigid Pendant##other##,Flexible Pendant##other##,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN
SAFJ03-S-04-GG-P,SAFJ03-S-04-GG-P,High Pressure Sodium,35,0.75,12,SAFJ03S04,JMP,JGL15,JGU15,generic,1,0,3000
SAFJ03-S-04-GG-P1,SAFJ03-S-04-GG-P1,High Pressure Sodium,35,1.00,12,SAFJ03S04,JMP1,JGL15,JGU15,generic,1,0,3000
SAFJ05-S-04-GG-P,SAFJ05-S-04-GG-P,High Pressure Sodium,50,0.75,13,SAFJ05S04,JMP,JGL15,JGU15,SAFJ05S.IES,1,0,3000
SAFJ05-S-04-GG-P1,SAFJ05-S-04-GG-P1,High Pressure Sodium,50,1.00,13,SAFJ05S04,JMP1,JGL15,JGU15,SAFJ05S.IES,1,0,3000
SAFJ07-S-04-GG-P,SAFJ07-S-04-GG-P,High Pressure Sodium,70,0.75,14,SAFJ07S04,JMP,JGL15,JGU15,SAFJ07S.IES,1,0,3000
SAFJ07-S-04-GG-P1,SAFJ07-S-04-GG-P1,High Pressure Sodium,70,1.00,14,SAFJ07S04,JMP1,JGL15,JGU15,SAFJ07S.IES,1,0,3000
SAFJ10-S-04-GG-P,SAFJ10-S-04-GG-P,High Pressure Sodium,100,0.75,16,SAFJ010S04,JMP,JGL15,JGU15,SAFJ10S.ies,1,0,3000
SAFJ10-S-04-GG-P1,SAFJ10-S-04-GG-P1,High Pressure Sodium,100,1.00,16,SAFJ010S04,JMP1,JGL15,JGU15,SAFJ10S.ies,1,0,3000
SAFJ03-S-04-GG-F,SAFJ03-S-04-GG-F,High Pressure Sodium,35,0.75,12,SAFJ03S04,JMF,JGL15,JGU15,generic,0,1,3000
SAFJ03-S-04-GG-F1,SAFJ03-S-04-GG-F1,High Pressure Sodium,35,1.00,12,SAFJ03S04,JMF1,JGL15,JGU15,generic,0,1,3000
SAFJ05-S-04-GG-F,SAFJ05-S-04-GG-F,High Pressure Sodium,50,0.75,13,SAFJ05S04,JMF,JGL15,JGU15,SAFJ05S.IES,0,1,3000
SAFJ05-S-04-GG-F1,SAFJ05-S-04-GG-F1,High Pressure Sodium,50,1.00,13,SAFJ05S04,JMF1,JGL15,JGU15,SAFJ05S.IES,0,1,3000
SAFJ07-S-04-GG-F,SAFJ07-S-04-GG-F,High Pressure Sodium,70,0.75,14,SAFJ07S04,JMF,JGL15,JGU15,SAFJ07S.IES,0,1,3000
SAFJ07-S-04-GG-F1,SAFJ07-S-04-GG-F1,High Pressure Sodium,70,1.00,14,SAFJ07S04,JMF1,JGL15,JGU15,SAFJ07S.IES,0,1,3000
SAFJ10-S-04-GG-F,SAFJ10-S-04-GG-F,High Pressure Sodium,100,0.75,16,SAFJ010S04,JMF,JGL15,JGU15,SAFJ10S.ies,0,1,3000
SAFJ10-S-04-GG-F1,SAFJ10-S-04-GG-F1,High Pressure Sodium,100,1.00,16,SAFJ010S04,JMF1,JGL15,JGU15,SAFJ10S.ies,0,1,3000
SAFJ05-H-04-GG-P,SAFJ05-H-04-GG-P,Metal Halide,50,0.75,14,SAFJ05H04,JMP,JGL15,JGU15,SAFJ05H.IES,1,0,4000
SAFJ05-H-04-GG-P1,SAFJ05-H-04-GG-P1,Metal Halide,50,1.00,14,SAFJ05H04,JMP1,JGL15,JGU15,SAFJ05H.IES,1,0,4000
SAFJ07-H-04-GG-P,SAFJ07-H-04-GG-P,Metal Halide,70,0.75,14,SAFJ07H04,JMP,JGL15,JGU15,SAFJ07H.IES,1,0,4000
SAFJ07-H-04-GG-P1,SAFJ07-H-04-GG-P1,Metal Halide,70,1.00,14,SAFJ07H04,JMP1,JGL15,JGU15,SAFJ07H.IES,1,0,4000
SAFJ10-H-04-GG-P,SAFJ10-H-04-GG-P,Metal Halide,100,0.75,15,SAFJ10H04,JMP,JGL15,JGU15,SAFJ10H.ies,1,0,4000
SAFJ10-H-04-GG-P1,SAFJ10-H-04-GG-P1,Metal Halide,100,1.00,15,SAFJ10H04,JMP1,JGL15,JGU15,SAFJ10H.ies,1,0,4000
SAFJ05-H-04-GG-F,SAFJ05-H-04-GG-F,Metal Halide,50,0.75,14,SAFJ05H04,JMP,JGL15,JGU15,SAFJ05H.IES,0,1,4000
SAFJ05-H-04-GG-F1,SAFJ05-H-04-GG-F1,Metal Halide,50,1.00,14,SAFJ05H04,JMP1,JGL15,JGU15,SAFJ05H.IES,0,1,4000
SAFJ07-H-04-GG-F,SAFJ07-H-04-GG-F,Metal Halide,70,0.75,14,SAFJ07H04,JMF,JGL15,JGU15,SAFJ07H.IES,0,1,4000
SAFJ07-H-04-GG-F1,SAFJ07-H-04-GG-F1,Metal Halide,70,1.00,14,SAFJ07H04,JMF1,JGL15,JGU15,SAFJ07H.IES,0,1,4000
SAFJ10-H-04-GG-F,SAFJ10-H-04-GG-F,Metal Halide,100,0.75,15,SAFJ10H04,JMF,JGL15,JGU15,SAFJ10H.ies,0,1,4000
SAFJ10-H-04-GG-F1,SAFJ10-H-04-GG-F1,Metal Halide,100,1.00,15,SAFJ10H04,JMF1,JGL15,JGU15,SAFJ10H.ies,0,1,4000
