,Catalog Number##other##,Lamp Type##other##,Wattage##other##,Conduit Size##Length##inches,Shipping Weight##other##,Ballast Housing##other##,Outlet Box##other##,Globe##other##,Guard##other##,Photometric Web File##other##,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN
03-S-04-GG-W,SAFJ05-H-04-GG-C,High Pressure Sodium,35,0.75,15,SAFJ03S04,JMW,JGL15,JGU15,generic,3000
03-S-04-GG-W1,SAFJ03-S-04-GG-W1,High Pressure Sodium,35,1.00,15,SAFJ03S04,JMW1,JGL15,JGU15,generic,3000
05-S-04-GG-W,SAFJ05-S-04-GG-W,High Pressure Sodium,50,0.75,16,SAFJ05S04,JMW,JGL15,JGU15,SAFJ05S.IES,3000
05-S-04-GG-W1,SAFJ05-S-04-GG-W1,High Pressure Sodium,50,1.00,16,SAFJ05S04,JMW1,JGL15,JGU15,SAFJ05S.IES,3000
07-S-04-GG-W,SAFJ07-S-04-GG-W,High Pressure Sodium,70,0.75,17,SAFJ07S04,JMW,JGL15,JGU15,SAFJ07S.IES,3000
07-S-04-GG-W1,SAFJ07-S-04-GG-W1,High Pressure Sodium,70,1.00,17,SAFJ07S04,JMW1,JGL15,JGU15,SAFJ07S.IES,3000
10-S-04-GG-W,SAFJ10-S-04-GG-W,High Pressure Sodium,100,0.75,18,SAFJ010S04,JMW,JGL15,JGU15,SAFJ10S.ies,3000
10-S-04-GG-W1,SAFJ10-S-04-GG-W1,High Pressure Sodium,100,1.00,18,SAFJ010S04,JMW1,JGL15,JGU15,SAFJ10S.ies,3000
05-H-04-GG-W,SAFJ05-H-04-GG-W,Metal Halide,50,0.75,17,SAFJ05H04,JMW,JGL15,JGU15,SAFJ05S.IES,4000
05-H-04-GG-W1,SAFJ05-H-04-GG-W1,Metal Halide,50,1.00,17,SAFJ05H04,JMW1,JGL15,JGU15,SAFJ05S.IES,4000
07-H-04-GG-W,SAFJ07-H-04-GG-W,Metal Halide,70,0.75,17,SAFJ07H04,JMW,JGL15,JGU15,SAFJ07S.IES,4000
07-H-04-GG-W1,SAFJ07-H-04-GG-W1,Metal Halide,70,1.00,17,SAFJ07H04,JMW1,JGL15,JGU15,SAFJ07S.IES,4000
10-H-04-GG-W,SAFJ10-H-04-GG-W,Metal Halide,100,0.75,18,SAFJ10H04,JMW,JGL15,JGU15,SAFJ10S.ies,4000
10-H-04-GG-W1,SAFJ10-H-04-GG-W1,Metal Halide,100,1.00,18,SAFJ10H04,JMW1,JGL15,JGU15,SAFJ10S.ies,4000
